BEECHCRAFT BARON 58
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 5,500 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VA - Maneuvering Speed | 156 KIAS
VLO - Maximum Gear Operating Speed | 152 KIAS
VLE - Maximum Landing Gear Extension Speed | 152 KIAS
Turbulent Air Penetration Speed | 156 KIAS
VNE - Never Exceed Speed | 223 KIAS
VS - Stalling Speed (maximum weight) | 84 KIAS
VSO - Stalling Speed in Landing Configuration | 75 KIAS
VX - Two-engine Best Angle-of-Climb Speed | 92 KIAS
VY - Two-engine Best Rate-of-Climb Speed | 105 KIAS
VXSE - Single-engine Best Angle-of-Climb Speed | 100 KIAS
VYSE - Single-engine Best Rate-of-Climb Speed | 101 KIAS
Minimum Icing Conditions Speed | 130 KIAS
VMCA - Minimum Control Speed | 84 KIAS
Minimum Glide Range Speed | 115 KIAS

Maximum Flap Placard Speeds

Flaps degrees | KIAS
15 | 152
30 | 122

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.