CESSNA SKYHAWK 172SP
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 2,550 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VA - Maneuvering Speed (2,550 lbs) | 105 KIAS
VA - Maneuvering Speed (2,200 lbs) | 98 KIAS
VA - Maneuvering Speed (1,900 lbs) | 90 KIAS
VNO - Max Structural Cruising Speed | 129 KIAS
VNE - Never Exceed Speed | 163 KIAS
VS - Stalling Speed (max weight, flaps up) | 48 KIAS
VSO - Stalling Speed in Landing Configuration | 40 KIAS
VX - Best Angle-of-Climb Speed (sea level) | 62 KIAS
VY - Best Rate-of-Climb Speed (sea level) | 74 KIAS
Best Glide Speed | 68 KIAS

Maximum Flap Placard Speeds

Flaps degrees | KIAS
10 | 110
15-30 | 85

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.